 Checking Master Surface   100 Versus Slave Surface   200

 Node:    26 Element:     3      3      4     15     14
 Node:    27 Element:     4      4      5     16     15
 Node:    28 Element:     5      5      6     17     16
 Node:    29 Element:     7      7      8     19     18
 Node:    30 Element:     8      8      9     20     19
 Warning -    5 Nodes penetrate master surface.
